Content

1 EZ220PU smart card reader installation

2 Reader Self Easy Check Function

3 Uninstall smart card reader

4 Direction for IC Card Insert

5 Led indicator

6 TROUBLE SHOOTING

# 1 EZ220PU Smart Card Reader Installation

## 1.1 Hardware Installation

Plug USB connector of Type A 4PIN into USB port of PC.

## 1.2 Driver Installation

Step (1): Plug the EZ220PU Smart Card Reader into your computer and Click the "Cancel" button if the "Add New Hardware Wizard" dialog appears.

Setp (2): Run "autorun.exe" of the setup disc or press "Install EZ220PU Driver".

Step (3): Click "Yes" button when the "EZ220PU Driver Setup" dialog appears.

Step (4): Click "Accept" button when the installer prompts you "Microsoft Smart Card Base Component"

Step (5): Click "Yes" button when the installer prompts you "Do you want to restart your computer now?"

Note: You can check the Smart Card Reader installed completely from the list of "Device Manager" after the system restart.

> > > 2 Reader Self Easy Check Function

> > > Step (1): Execute Programs/EZ220PU Utility/EZ220PU Diagnostics

> > > Step (2): Press "Diagnostic" button to execute Self Easy Check Function.

> > > Step (3): When all items had been checked in "PASSED" field that means the Smart Card Reader had been installed successfully. Please press "Exit" button to finish this program.

# 3 Uninstall Smart Card Reader

Step (1): Execute Programs/EZ220PU Utility/Uninstall EZ220PU Reader

Step (2): When the dialog display "Are you sure that you want to remove EZ220PU Smart Card Reader?", please press "Yes" to remove reader. Otherwise, press "No" button to close this dialog.

Step (3): When the Smart Card had been removed successfully. The dialog will display message as follows. Please press "OK" button to close this dialog.

# 4 Direction for IC Card Insert

EZ220PU

# 5 LED Indicator

- # Yellow-Green Light : Smart Card Reader had been power on.

- # Red Light : IC Card has been reset. When red light is in flashing that means IC Card is processing reading or writing.

6 Trouble Shooting

Trouble s hooting please refer to EZ PC/SC Reader FAQ for detail.